IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2019-08-14T10:59:37"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_1515(x64) - Exporter 2015.0.2016.0512 - Default UI"
Application: "Autodesk Revit 2015 (DEU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (DEU)"

People and organizations
  Person "Tilo110663" of Organization (no name given)
  Owner history of Person "Tilo110663" of Organization (no name given) | application "Autodesk Revit 2015 (DEU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "C:\Users\Tilo110663\Desktop\Coolkompakt\CoolKompakt\CuC_Final\10-Kühlwannen\3-Kühlwanne stille Kühlung GN1-1\KWOS031100.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "3xGN1-1" | names: "Kühlwanne stille Kühlung GN1-1 - Zentral:3xGN1-1:14508" | material: "Edelstahl AISI 304" | property sets: Pset_BuildingElementProxyCommon, Abhängigkeiten, Abmessungen, Elektro - Lasten, Phasen, Sonstige

Property sets
  Sonstige | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Kategorie = "Projektinformationen" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Familienname = "Ebene" (IFCTEXT)
    Kategorie = "Ebenen" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Familie = "Kühlwanne stille Kühlung GN1-1 - Zentral: 3xGN1-1" (IFCLABEL)
    Familie und Typ = "Kühlwanne stille Kühlung GN1-1 - Zentral: 3xGN1-1" (IFCLABEL)
    Kategorie = "Sonderausstattung" (IFCLABEL)
    Typ = "Kühlwanne stille Kühlung GN1-1 - Zentral: 3xGN1-1" (IFCLABEL)
    Typ-ID = "Kühlwanne stille Kühlung GN1-1 - Zentral: 3xGN1-1" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Familie = "Ebene: Ebene 1" (IFCLABEL)
    Familie und Typ = "Ebene: Ebene 1" (IFCLABEL)
    Kategorie = "Ebenen" (IFCLABEL)
    Typ = "Ebene: Ebene 1" (IFCLABEL)
    Typ-ID = "Ebene: Ebene 1" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Familienname = "Kühlwanne stille Kühlung GN1-1 - Zentral" (IFCTEXT)
    Kapazität = "3 x GN 1/1, Tiefe 30 - 200 mm" (IFCTEXT)
    Kategorie = "Sonderausstattung" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "3xGN1-1" (IFCIDENTIFIER)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 1" (IFCTEXT)
    Ebene = "Ebene: Ebene 1" (IFCLABEL)
    Installationshöhe = 750. (IFCLENGTHMEASURE) [MILLI METRE]
    Versatz = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Fläche = 1.43841283085421 (IFCAREAMEASURE) [SQUARE_METRE]
    Volumen = 0.195065935000018 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Breite = 1135. (IFCLENGTHMEASURE) [MILLI METRE]
    Breite Technikgehäuse = 442. (IFCLENGTHMEASURE) [MILLI METRE]
    Breite ohne Rahmen = 1091. (IFCLENGTHMEASURE) [MILLI METRE]
    Höhe = 380. (IFCLENGTHMEASURE) [MILLI METRE]
    Höhe Technikgehäuse = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Höhe Wanne = 270. (IFCLENGTHMEASURE) [MILLI METRE]
    Tiefe = 635. (IFCLENGTHMEASURE) [MILLI METRE]
    Tiefe ohne Rahmen = 590. (IFCLENGTHMEASURE) [MILLI METRE]
  Elektro - Lasten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Element = "" (IFCTEXT)
    Stromkreisnummer = "" (IFCTEXT)
  Phasen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Neue Konstruktion" (IFCLABEL)
  ID-Daten | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Artikelnr. = "KWOS031100" (IFCTEXT)
    Baugruppenbeschreibung = "" (IFCTEXT)
    Baugruppenkennzeichen = "" (IFCTEXT)
    OmniClass-Nummer = "" (IFCTEXT)
    OmniClass-Titel = "" (IFCTEXT)
    Typname = "3xGN1-1" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Typname = "Ebene 1" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Elektro | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pole = 1 (IFCINTEGER)
    Scheinleistung = 0. (IFCPOWERMEASURE) [WATT]
    Spannung = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Watt = 40. (IFCPOWERMEASURE) [WATT]
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    DN Flüssigkeitsleitung = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    DN Saugleitung = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    DN Tauwasserabfluß = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Kälteleistung = "1050 W / -10°C VT" (IFCTEXT)
    Kältemittel = "R404a" (IFCTEXT)
    Temp. Bereich = "4°C bis +10°C" (IFCTEXT)
  Konstruktion | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Boden Stärke = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Rand Breite hinten = 62.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Rand Breite seitlich = 87.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Rand Breite vorne = 62.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Rand Stärke = 8.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Wand Seiten Stärke = 65.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Wand hinten Stärke = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Wand vorne Stärke = 40. (IFCLENGTHMEASURE) [MILLI METRE]
  Materialien und Oberflächen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Material = "Edelstahl AISI 304" (IFCLABEL)
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 0 (IFCINTEGER)
    Linienmuster = "Kompakt" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)